(footprint "WDFN-6-2EP_4.0x2.6mm_P0.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "WDFN, 6 pin, 4.0x2.6, 0.65P; Two exposed pads, (https://www.onsemi.com/pub/Collateral/511BZ.PDF)")
	(tags "DFN 0.65P dual flag")
	(property "Reference" "REF**"
		(at 0 -2.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "WDFN-6-2EP_4.0x2.6mm_P0.65mm"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.9 -0.65 270)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.9 0 270)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.9 0.65 270)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.9 0.65 270)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.9 0 270)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.9 -0.65 270)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0 -0.438 270)
		(size 1.415 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0 0.838 270)
		(size 0.615 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WDFN-6-2EP_4.0x2.6mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
