(footprint "WDFN-8-1EP_8x6mm_P1.27mm_EP6x4.8mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "WDFN, 8 Pin (https://ww1.microchip.com/downloads/en/DeviceDoc/8L_WDFN_6x8mm_MN_C04172A.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "WDFN NoLead Microchip-8L-WDFN-6x8mm-MN-C04172A")
	(property "Reference" "REF**"
		(at 0 -3.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "WDFN-8-1EP_8x6mm_P1.27mm_EP6x4.8mm_ThermalVias"
		(at 0 3.95 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -2.01375 -1.39)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at -2.01375 0)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at -2.01375 1.39)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at -0.67125 -1.39)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at -0.67125 0)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at -0.67125 1.39)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at 0.67125 -1.39)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at 0.67125 0)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at 0.67125 1.39)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at 2.01375 -1.39)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at 2.01375 0)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "" smd custom
		(at 2.01375 1.39)
		(size 1.026787 1.026787)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.422118 -0.311199)
					(xy -0.270888 -0.462429)
					(xy 0.270888 -0.462429)
					(xy 0.422118 -0.311199)
					(xy 0.422118 0.311199)
					(xy 0.270888 0.462429)
					(xy -0.270888 0.462429)
					(xy -0.422118 0.311199)
				)
				(width 0.365103)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.9 -1.905)
		(size 0.9 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.9 -0.635)
		(size 0.9 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.9 0.635)
		(size 0.9 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.9 1.905)
		(size 0.9 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.9 1.905)
		(size 0.9 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 3.9 0.635)
		(size 0.9 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 3.9 -0.635)
		(size 0.9 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 3.9 -1.905)
		(size 0.9 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" thru_hole circle
		(at -2.685 -2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -2.685 -0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -2.685 0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -2.685 2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -1.3425 -2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -1.3425 -0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -1.3425 0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -1.3425 2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 -2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 -0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 6 4.8)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 6 4.8)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "9" thru_hole circle
		(at 0 0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 1.3425 -2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 1.3425 -0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 1.3425 0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 1.3425 2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2.685 -2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2.685 -0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2.685 0.695)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2.685 2.085)
		(size 0.63 0.63)
		(drill 0.33)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WDFN-8-1EP_8x6mm_P1.27mm_EP6x4.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
