(footprint "WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.onsemi.com/pub/Collateral/510CD.PDF")
	(tags "WQFN-20 4.5mm 2.5mm 0.5mm")
	(property "Reference" "REF**"
		(at 0 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at 0 -0.95 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0.95 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -0.25 -2.3 270)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.3 -1.75)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.3 -1.25)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.3 -0.75)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.3 -0.25)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.3 0.25)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.3 0.75)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -1.3 1.25)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.3 1.75)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -0.25 2.3 270)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.25 2.3 270)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.3 1.75)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.3 1.25)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.3 0.75)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 1.3 0.25)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.3 -0.25)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 1.3 -0.75)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.3 -1.25)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.3 -1.75)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 0.25 -2.3 270)
		(size 0.9 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0 0 270)
		(size 2.9 1)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
