(footprint "DIP-5-6_W7.62mm_SMDSocket_SmallPads"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads")
	(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads")
	(property "Reference" "REF**"
		(at 0 -4.87 0)
		(layer "F.SilkS")
	)
	(property "Value" "DIP-5-6_W7.62mm_SMDSocket_SmallPads"
		(at 0 4.87 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.81 -2.54)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.81 0)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.81 2.54)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.81 2.54)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3.81 -2.54)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-5-6_W7.62mm_SMDSocket.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
