(footprint "Fairchild_LSOP-8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-Lead, 300\\\" Wide, Surface Mount Package (https://www.fairchildsemi.com/package-drawings/ML/MLSOP08A.pdf)")
	(tags "LSOP 2.54mm 300mil")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fairchild_LSOP-8"
		(at 0 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.35 -3.81)
		(size 2 1.252)
		(drill
			(offset 0 0.266)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.35 -1.27)
		(size 2 1.784)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.35 1.27)
		(size 2 1.784)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.35 3.81)
		(size 2 1.252)
		(drill
			(offset 0 -0.266)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 4.35 3.81)
		(size 2 1.252)
		(drill
			(offset 0 -0.266)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 4.35 1.27)
		(size 2 1.784)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 4.35 -1.27)
		(size 2 1.784)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.35 -3.81)
		(size 2 1.252)
		(drill
			(offset 0 0.266)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/Fairchild_LSOP-8.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
