(footprint "SMDIP-4_W9.53mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "4-lead surface-mounted (SMD) DIP package, row spacing 9.53mm (375 mils)")
	(tags "SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil")
	(property "Reference" "REF**"
		(at 0 -3.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "SMDIP-4_W9.53mm"
		(at 0 3.6 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.765 -1.27)
		(size 2 1.78)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.140449)
	)
	(pad "2" smd roundrect
		(at -4.765 1.27)
		(size 2 1.78)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.140449)
	)
	(pad "3" smd roundrect
		(at 4.765 1.27)
		(size 2 1.78)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.140449)
	)
	(pad "4" smd roundrect
		(at 4.765 -1.27)
		(size 2 1.78)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.140449)
	)
	(model "${KICAD9_3DMODEL_DIR}/Housings_DIP.3dshapes/SMDIP-4_W9.53mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
