(footprint "DirectFET_L4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DirectFET L4 https://www.infineon.com/dgdl/Infineon-AN-1035-ApplicationNotes-v29_01-EN.pdf?fileId=5546d462533600a40153559159020f76#page=41")
	(tags "DirectFET L4 MOSFET Infineon")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "DirectFET_L4"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.5 -2.2)
		(size 1.1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -4.5 0)
		(size 1.1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -4.5 2.2)
		(size 1.1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 4.5 -2.2)
		(size 1.1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 4.5 0)
		(size 1.1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 4.5 2.2)
		(size 1.1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.25 0)
		(size 0.7 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.85 -0.575)
		(size 1.1 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.85 0.575)
		(size 1.1 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.55 -0.575)
		(size 1.1 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.55 0.575)
		(size 1.1 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DirectFET.3dshapes/DirectFET_L4.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
