(footprint "Analog_LCC-8_5x5mm_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LCC, ceramic leaded chip carrier, 8 pins, surface mount, Analog Devices LS8, 5x5mm, height 1.45mm, https://www.analog.com/media/en/technical-documentation/data-sheets/ltc6655-6655ln.pdf")
	(tags "lcc smt")
	(property "Reference" "REF**"
		(at -0.8 -4.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Analog_LCC-8_5x5mm_P1.27mm"
		(at -0.1 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.15 -1.27 90)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.15 0 90)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.15 1.27 90)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0 2.15 90)
		(size 1.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.15 1.27)
		(size 1.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.15 0)
		(size 1.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.15 -1.27)
		(size 1.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0 -1.75 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LCC.3dshapes/Analog_LCC-8_5x5mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
