(footprint "PLCC-84_THT-Socket"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PLCC, 84 pins, through hole")
	(tags "plcc leaded")
	(property "Reference" "REF**"
		(at 0 -3.77 0)
		(layer "F.SilkS")
	)
	(property "Value" "PLCC-84_THT-Socket"
		(at 0 34.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 15.24 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -2.54 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.54 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -5.08 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -5.08 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at -7.62 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at -7.62 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -10.16 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at -10.16 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at -12.7 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at -15.24 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -12.7 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at -15.24 5.08)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at -12.7 5.08)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at -15.24 7.62)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at -12.7 7.62)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at -15.24 10.16)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at -12.7 10.16)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at -15.24 12.7)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -12.7 12.7)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at -15.24 15.24)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at -12.7 15.24)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at -15.24 17.78)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at -12.7 17.78)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole circle
		(at -15.24 20.32)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at -12.7 20.32)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole circle
		(at -15.24 22.86)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at -12.7 22.86)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" thru_hole circle
		(at -15.24 25.4)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" thru_hole circle
		(at -12.7 25.4)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "32" thru_hole circle
		(at -15.24 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at -12.7 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at -12.7 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "35" thru_hole circle
		(at -10.16 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "36" thru_hole circle
		(at -10.16 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at -7.62 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "38" thru_hole circle
		(at -7.62 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at -5.08 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "40" thru_hole circle
		(at -5.08 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at -2.54 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "42" thru_hole circle
		(at -2.54 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "44" thru_hole circle
		(at 0 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "45" thru_hole circle
		(at 2.54 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "46" thru_hole circle
		(at 2.54 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "47" thru_hole circle
		(at 5.08 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "48" thru_hole circle
		(at 5.08 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 7.62 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "50" thru_hole circle
		(at 7.62 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "51" thru_hole circle
		(at 10.16 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "52" thru_hole circle
		(at 10.16 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "53" thru_hole circle
		(at 12.7 30.48)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "54" thru_hole circle
		(at 15.24 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "55" thru_hole circle
		(at 12.7 27.94)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "56" thru_hole circle
		(at 15.24 25.4)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 12.7 25.4)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "58" thru_hole circle
		(at 15.24 22.86)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "59" thru_hole circle
		(at 12.7 22.86)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "60" thru_hole circle
		(at 15.24 20.32)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "61" thru_hole circle
		(at 12.7 20.32)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "62" thru_hole circle
		(at 15.24 17.78)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "63" thru_hole circle
		(at 12.7 17.78)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "64" thru_hole circle
		(at 15.24 15.24)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "65" thru_hole circle
		(at 12.7 15.24)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "66" thru_hole circle
		(at 15.24 12.7)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "67" thru_hole circle
		(at 12.7 12.7)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "68" thru_hole circle
		(at 15.24 10.16)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 12.7 10.16)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "70" thru_hole circle
		(at 15.24 7.62)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "71" thru_hole circle
		(at 12.7 7.62)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "72" thru_hole circle
		(at 15.24 5.08)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 12.7 5.08)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "74" thru_hole circle
		(at 15.24 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "75" thru_hole circle
		(at 12.7 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "76" thru_hole circle
		(at 12.7 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "77" thru_hole circle
		(at 10.16 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "78" thru_hole circle
		(at 10.16 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "79" thru_hole circle
		(at 7.62 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "80" thru_hole circle
		(at 7.62 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "81" thru_hole circle
		(at 5.08 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "82" thru_hole circle
		(at 5.08 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "83" thru_hole circle
		(at 2.54 0)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "84" thru_hole circle
		(at 2.54 2.54)
		(size 1.4224 1.4224)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LCC.3dshapes/PLCC-84_THT-Socket.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
