(footprint "AMS_OLGA-8_2x3.1mm_P0.8mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "AMS  OLGA, 8 Pin (https://ams.com/documents/20143/36005/AS7341_DS000504_3-00.pdf/#page=63)")
	(tags "AMS OLGA NoLead")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "AMS_OLGA-8_2x3.1mm_P0.8mm"
		(at 0 2.6 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.25 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.638 -1.2)
		(size 0.575 0.488)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.3625)
		(chamfer bottom_right)
	)
	(pad "2" smd rect
		(at -0.638 -0.4)
		(size 0.575 0.488)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.638 0.4)
		(size 0.575 0.488)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.638 1.2)
		(size 0.575 0.488)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.638 1.2)
		(size 0.575 0.488)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.638 0.4)
		(size 0.575 0.488)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.638 -0.4)
		(size 0.575 0.488)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.638 -1.2)
		(size 0.575 0.488)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/AMS_OLGA-8_2x3.1mm_P0.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
