(footprint "Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LGA-8")
	(tags "lga land grid array")
	(property "Reference" "REF**"
		(at 0.015 -2.465 0)
		(layer "F.SilkS")
	)
	(property "Value" "Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering"
		(at 0.015 2.535 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.975 -1.025 90)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.325 -1.025 90)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.325 -1.025 90)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.975 -1.025 90)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.975 1.025 90)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.325 1.025 90)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.325 1.025 90)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -0.975 1.025 90)
		(size 0.5 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering.wrl"
		(offset
			(xyz 0.01500000025 -0.03500000059 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
