(footprint "LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "LGA, 16 Pin (http://www.st.com/resource/en/datasheet/lis331hh.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "LGA NoLead")
	(property "Reference" "REF**"
		(at 0 -2.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y"
		(at 0 2.45 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.225 -1)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.225 -0.5)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.225 0)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.225 0.5)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.225 1)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -0.5 1.225)
		(size 0.35 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0 1.225)
		(size 0.35 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.5 1.225)
		(size 0.35 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.225 1)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.225 0.5)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.225 0)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.225 -0.5)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.225 -1)
		(size 0.55 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 0.5 -1.225)
		(size 0.35 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 0 -1.225)
		(size 0.35 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -0.5 -1.225)
		(size 0.35 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
