(footprint "LGA-24L_3x3.5mm_P0.43mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LGA 24L 3x3.5mm Pitch 0.43mm")
	(tags "LGA 24L 3x3.5mm Pitch 0.43mm")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "LGA-24L_3x3.5mm_P0.43mm"
		(at 0 2.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -2.7 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.505 -1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.475 -0.645)
		(size 0.35 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.475 -0.215)
		(size 0.35 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.475 0.215)
		(size 0.35 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.475 0.645)
		(size 0.35 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.505 1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.075 1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -0.645 1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -0.215 1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.215 1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.645 1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.075 1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.505 1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.475 0.645)
		(size 0.35 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 1.475 0.215)
		(size 0.35 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.475 -0.215)
		(size 0.35 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 1.475 -0.645)
		(size 0.35 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.505 -1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.075 -1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 0.645 -1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0.215 -1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -0.215 -1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -0.645 -1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -1.075 -1.225)
		(size 0.23 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-24L_3x3.5mm_P0.43mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
