(footprint "MPS_LGA-18-10EP_12x12mm_P3.3mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MPS LGA-18 12x12x3.82mm (https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MPM3550EGLE/document_id/5102/)")
	(tags "MPS LGA")
	(property "Reference" "REF**"
		(at 0 -7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "MPS_LGA-18-10EP_12x12mm_P3.3mm"
		(at 0 7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.95 -4.95)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -4.95 -1.65)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -4.95 1.65)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -4.95 4.95)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at 4.95 4.95)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at 4.95 1.65)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at 4.95 -1.65)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 4.95 -4.95)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at 1.15 -4.8)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 1.15 -2.4)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at 1.15 0)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at 1.15 2.4)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at 1.15 4.8)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at -1.15 4.8)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at -1.15 2.4)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd roundrect
		(at -1.15 0)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd roundrect
		(at -1.15 -2.4)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd roundrect
		(at -1.15 -4.8)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/MPS_LGA-18-10EP_12x12mm_P3.3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
