(footprint "ST_CCLGA-7L_2.8x2.8mm_P1.15mm_H1.95mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ST  CCLGA, 7 Pin (https://www.st.com/resource/en/datasheet/ilps28qsw.pdf#page=44)")
	(tags "water resistant package")
	(property "Reference" "REF**"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "ST_CCLGA-7L_2.8x2.8mm_P1.15mm_H1.95mm"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at 0 -1.125)
		(size 1.4 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
		(chamfer_ratio 0.3)
		(chamfer bottom_right)
	)
	(pad "2" smd roundrect
		(at -1.125 -0.575 90)
		(size 0.9 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "3" smd roundrect
		(at -1.125 0.575 90)
		(size 0.9 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "4" smd roundrect
		(at 0 1.125)
		(size 1.4 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "5" smd roundrect
		(at 1.125 0.575 90)
		(size 0.9 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "6" smd roundrect
		(at 1.125 -0.575 90)
		(size 0.9 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(pad "7" smd roundrect
		(at 0 0)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/ST_CCLGA-7L_2.8x2.8mm_P1.15mm_H1.95mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
