(footprint "ST_HLGA-10_2.5x2.5mm_P0.6mm_LayoutBorder3x2y"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ST  HLGA, 10 Pin (https://www.st.com/resource/en/datasheet/lps25hb.pdf#page=46), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "ST HLGA NoLead")
	(property "Reference" "REF**"
		(at 0 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_HLGA-10_2.5x2.5mm_P0.6mm_LayoutBorder3x2y"
		(at 0 2.2 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.925 -0.3)
		(size 0.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.925 0.3)
		(size 0.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.6 0.925)
		(size 0.4 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0 0.925)
		(size 0.4 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.6 0.925)
		(size 0.4 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.925 0.3)
		(size 0.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.925 -0.3)
		(size 0.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.6 -0.925)
		(size 0.4 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0 -0.925)
		(size 0.4 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.6 -0.925)
		(size 0.4 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/ST_HLGA-10_2.5x2.5mm_P0.6mm_LayoutBorder3x2y.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
