(footprint "Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas SIL0010A MicroSiP, 10 Pin (http://www.ti.com/lit/ml/mpds579b/mpds579b.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "Texas MicroSiP NoLead")
	(property "Reference" "REF**"
		(at 0 -2.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm_ThermalVias"
		(at 0 2.45 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.175 -0.97)
		(size 0.65 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.175 0)
		(size 0.65 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.175 0.97)
		(size 0.65 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.525 -1.2)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.525 -0.6)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.525 0)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.525 0.6)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.525 1.2)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 1.525 1.2)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1.525 0.6)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.525 0)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.525 -0.6)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.525 -1.2)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" thru_hole circle
		(at -0.175 -1.03)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at -0.175 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "11" smd rect
		(at -0.175 0)
		(size 0.5 2.56)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "11" smd rect
		(at -0.175 0)
		(size 0.7 2.9)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "11" thru_hole circle
		(at -0.175 1.03)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
