(footprint "LQFP-48-1EP_7x7mm_P0.5mm_EP3.6x3.6mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "LQFP, 48 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "LQFP QFP")
	(property "Reference" "REF**"
		(at 0 -5.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "LQFP-48-1EP_7x7mm_P0.5mm_EP3.6x3.6mm_ThermalVias"
		(at 0 5.85 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.4 -1.4)
		(size 0.554596 0.554596)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.232106 -0.232106)
					(xy 0.232106 -0.232106)
					(xy 0.232106 0.157228)
					(xy 0.157228 0.232106)
					(xy -0.232106 0.232106)
				)
				(width 0.180769)
			)
		)
	)
	(pad "" smd custom
		(at -1.4 -0.5)
		(size 0.568298 0.568298)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.245807 -0.32643)
					(xy 0.182281 -0.32643)
					(xy 0.245807 -0.262904)
					(xy 0.245807 0.262904)
					(xy 0.182281 0.32643)
					(xy -0.245807 0.32643)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at -1.4 0.5)
		(size 0.568298 0.568298)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.245807 -0.32643)
					(xy 0.182281 -0.32643)
					(xy 0.245807 -0.262904)
					(xy 0.245807 0.262904)
					(xy 0.182281 0.32643)
					(xy -0.245807 0.32643)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at -1.4 1.4)
		(size 0.554596 0.554596)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.232106 -0.232106)
					(xy 0.157228 -0.232106)
					(xy 0.232106 -0.157228)
					(xy 0.232106 0.232106)
					(xy -0.232106 0.232106)
				)
				(width 0.180769)
			)
		)
	)
	(pad "" smd custom
		(at -0.5 -1.4)
		(size 0.568298 0.568298)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.32643 -0.245807)
					(xy 0.32643 -0.245807)
					(xy 0.32643 0.182281)
					(xy 0.262904 0.245807)
					(xy -0.262904 0.245807)
					(xy -0.32643 0.182281)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd roundrect
		(at -0.5 -0.5)
		(size 0.806226 0.806226)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.5 0.5)
		(size 0.806226 0.806226)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at -0.5 1.4)
		(size 0.568298 0.568298)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.32643 -0.182281)
					(xy -0.262904 -0.245807)
					(xy 0.262904 -0.245807)
					(xy 0.32643 -0.182281)
					(xy 0.32643 0.245807)
					(xy -0.32643 0.245807)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 0.5 -1.4)
		(size 0.568298 0.568298)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.32643 -0.245807)
					(xy 0.32643 -0.245807)
					(xy 0.32643 0.182281)
					(xy 0.262904 0.245807)
					(xy -0.262904 0.245807)
					(xy -0.32643 0.182281)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd roundrect
		(at 0.5 -0.5)
		(size 0.806226 0.806226)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.5 0.5)
		(size 0.806226 0.806226)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at 0.5 1.4)
		(size 0.568298 0.568298)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.32643 -0.182281)
					(xy -0.262904 -0.245807)
					(xy 0.262904 -0.245807)
					(xy 0.32643 -0.182281)
					(xy 0.32643 0.245807)
					(xy -0.32643 0.245807)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 1.4 -1.4)
		(size 0.554596 0.554596)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.232106 -0.232106)
					(xy 0.232106 -0.232106)
					(xy 0.232106 0.232106)
					(xy -0.157228 0.232106)
					(xy -0.232106 0.157228)
				)
				(width 0.180769)
			)
		)
	)
	(pad "" smd custom
		(at 1.4 -0.5)
		(size 0.568298 0.568298)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.245807 -0.262904)
					(xy -0.182281 -0.32643)
					(xy 0.245807 -0.32643)
					(xy 0.245807 0.32643)
					(xy -0.182281 0.32643)
					(xy -0.245807 0.262904)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 1.4 0.5)
		(size 0.568298 0.568298)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.245807 -0.262904)
					(xy -0.182281 -0.32643)
					(xy 0.245807 -0.32643)
					(xy 0.245807 0.32643)
					(xy -0.182281 0.32643)
					(xy -0.245807 0.262904)
				)
				(width 0.153366)
			)
		)
	)
	(pad "" smd custom
		(at 1.4 1.4)
		(size 0.554596 0.554596)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.232106 -0.157228)
					(xy -0.157228 -0.232106)
					(xy 0.232106 -0.232106)
					(xy 0.232106 0.232106)
					(xy -0.232106 0.232106)
				)
				(width 0.180769)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.1625 -2.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.1625 -2.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.1625 -1.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -4.1625 -1.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -4.1625 -0.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -4.1625 -0.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -4.1625 0.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -4.1625 0.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -4.1625 1.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -4.1625 1.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -4.1625 2.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -4.1625 2.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -2.75 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -2.25 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -1.75 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -1.25 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -0.75 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -0.25 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 0.25 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 0.75 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 1.25 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.75 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 2.25 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.75 4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 4.1625 2.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 4.1625 2.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 4.1625 1.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 4.1625 1.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 4.1625 0.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 4.1625 0.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 4.1625 -0.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 4.1625 -0.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 4.1625 -1.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 4.1625 -1.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 4.1625 -2.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 4.1625 -2.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 2.75 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 2.25 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 1.75 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 1.25 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 0.75 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 0.25 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at -0.25 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at -0.75 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at -1.25 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at -1.75 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at -2.25 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at -2.75 -4.1625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "49" thru_hole circle
		(at -1 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at -1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at -1 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 0 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" smd rect
		(at 0 0)
		(size 2.5 2.5)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "49" smd rect
		(at 0 0)
		(size 3.6 3.6)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "49" thru_hole circle
		(at 0 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 1 -1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 1 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 1 1)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-48-1EP_7x7mm_P0.5mm_EP3.6x3.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
