(footprint "LQFP-52-1EP_10x10mm_P0.65mm_EP4.8x4.8mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "LQFP, 52 Pin (https://www.onsemi.com/pub/Collateral/848H-01.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "LQFP QFP")
	(property "Reference" "REF**"
		(at 0 -7.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "LQFP-52-1EP_10x10mm_P0.65mm_EP4.8x4.8mm"
		(at 0 7.35 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.6 -1.6)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "" smd roundrect
		(at -1.6 0)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "" smd roundrect
		(at -1.6 1.6)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "" smd roundrect
		(at 0 -1.6)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "" smd roundrect
		(at 0 1.6)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "" smd roundrect
		(at 1.6 -1.6)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "" smd roundrect
		(at 1.6 0)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "" smd roundrect
		(at 1.6 1.6)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
	)
	(pad "1" smd roundrect
		(at -5.6625 -3.9)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -5.6625 -3.25)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -5.6625 -2.6)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -5.6625 -1.95)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -5.6625 -1.3)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -5.6625 -0.65)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -5.6625 0)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -5.6625 0.65)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -5.6625 1.3)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -5.6625 1.95)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -5.6625 2.6)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -5.6625 3.25)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -5.6625 3.9)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -3.9 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -3.25 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -2.6 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -1.95 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -1.3 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -0.65 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 0 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 0.65 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.3 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1.95 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.6 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 3.25 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 3.9 5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 5.6625 3.9)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 5.6625 3.25)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 5.6625 2.6)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 5.6625 1.95)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 5.6625 1.3)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 5.6625 0.65)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 5.6625 0)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 5.6625 -0.65)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 5.6625 -1.3)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 5.6625 -1.95)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 5.6625 -2.6)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 5.6625 -3.25)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 5.6625 -3.9)
		(size 1.475 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 3.9 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 3.25 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 2.6 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 1.95 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at 1.3 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 0.65 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 0 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at -0.65 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at -1.3 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at -1.95 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at -2.6 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at -3.25 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at -3.9 -5.6625)
		(size 0.4 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd rect
		(at 0 0)
		(size 4.8 4.8)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-52-1EP_10x10mm_P0.65mm_EP4.8x4.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
