(footprint "PQFP-132_24x24mm_P0.635mm_i386"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PQFP, 132 pins, 24mm sq body, 0.635mm pitch, Intel 386EX (https://www.intel.com/content/dam/www/public/us/en/documents/packaging-databooks/packaging-chapter-02-databook.pdf, http://www.nxp.com/docs/en/application-note/AN4388.pdf)")
	(tags "PQFP 132 Intel 386EX")
	(property "Reference" "REF**"
		(at 0 -15.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "PQFP-132_24x24mm_P0.635mm_i386"
		(at 0 15.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -13.4 -10.16)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -13.4 -9.525)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -13.4 -8.89)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -13.4 -8.255)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -13.4 -7.62)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -13.4 -6.985)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -13.4 -6.35)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -13.4 -5.715)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -13.4 -5.08)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -13.4 -4.445)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -13.4 -3.81)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -13.4 -3.175)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -13.4 -2.54)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -13.4 -1.905)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -13.4 -1.27)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -13.4 -0.635)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -13.4 0)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -13.4 0.635)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -13.4 1.27)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -13.4 1.905)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -13.4 2.54)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -13.4 3.175)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -13.4 3.81)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -13.4 4.445)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -13.4 5.08)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -13.4 5.715)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -13.4 6.35)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -13.4 6.985)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -13.4 7.62)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -13.4 8.255)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -13.4 8.89)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -13.4 9.525)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -13.4 10.16)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -10.16 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -9.525 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -8.89 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -8.255 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at -7.62 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -6.985 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -6.35 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -5.715 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at -5.08 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -4.445 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -3.81 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -3.175 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -2.54 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -1.905 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -1.27 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at -0.635 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 0 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 0.635 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 1.27 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 1.905 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 2.54 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 3.175 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 3.81 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 4.445 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at 5.08 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at 5.715 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at 6.35 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at 6.985 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at 7.62 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at 8.255 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at 8.89 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at 9.525 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at 10.16 13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at 13.4 10.16)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at 13.4 9.525)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at 13.4 8.89)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at 13.4 8.255)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at 13.4 7.62)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at 13.4 6.985)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at 13.4 6.35)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at 13.4 5.715)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at 13.4 5.08)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at 13.4 4.445)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at 13.4 3.81)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at 13.4 3.175)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at 13.4 2.54)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at 13.4 1.905)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at 13.4 1.27)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at 13.4 0.635)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at 13.4 0)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at 13.4 -0.635)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at 13.4 -1.27)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at 13.4 -1.905)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd rect
		(at 13.4 -2.54)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd rect
		(at 13.4 -3.175)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd rect
		(at 13.4 -3.81)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd rect
		(at 13.4 -4.445)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd rect
		(at 13.4 -5.08)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd rect
		(at 13.4 -5.715)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd rect
		(at 13.4 -6.35)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd rect
		(at 13.4 -6.985)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd rect
		(at 13.4 -7.62)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd rect
		(at 13.4 -8.255)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd rect
		(at 13.4 -8.89)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd rect
		(at 13.4 -9.525)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd rect
		(at 13.4 -10.16)
		(size 1.635 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd rect
		(at 10.16 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd rect
		(at 9.525 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd rect
		(at 8.89 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd rect
		(at 8.255 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd rect
		(at 7.62 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd rect
		(at 6.985 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd rect
		(at 6.35 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd rect
		(at 5.715 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd rect
		(at 5.08 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd rect
		(at 4.445 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd rect
		(at 3.81 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd rect
		(at 3.175 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd rect
		(at 2.54 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd rect
		(at 1.905 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd rect
		(at 1.27 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd rect
		(at 0.635 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd rect
		(at 0 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd rect
		(at -0.635 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd rect
		(at -1.27 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd rect
		(at -1.905 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd rect
		(at -2.54 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd rect
		(at -3.175 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd rect
		(at -3.81 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd rect
		(at -4.445 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd rect
		(at -5.08 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd rect
		(at -5.715 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "126" smd rect
		(at -6.35 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "127" smd rect
		(at -6.985 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "128" smd rect
		(at -7.62 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "129" smd rect
		(at -8.255 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "130" smd rect
		(at -8.89 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "131" smd rect
		(at -9.525 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "132" smd rect
		(at -10.16 -13.4)
		(size 0.38 1.635)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-132_24x24mm_P0.635mm_i386.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
