(footprint "PQFP-208_28x28mm_P0.5mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "PQFP, 208 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "PQFP QFP")
	(property "Reference" "REF**"
		(at 0 -16.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "PQFP-208_28x28mm_P0.5mm"
		(at 0 16.65 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -14.9625 -12.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -14.9625 -12.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -14.9625 -11.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -14.9625 -11.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -14.9625 -10.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -14.9625 -10.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -14.9625 -9.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -14.9625 -9.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -14.9625 -8.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -14.9625 -8.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -14.9625 -7.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -14.9625 -7.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -14.9625 -6.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -14.9625 -6.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -14.9625 -5.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -14.9625 -5.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -14.9625 -4.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -14.9625 -4.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -14.9625 -3.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -14.9625 -3.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -14.9625 -2.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -14.9625 -2.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -14.9625 -1.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -14.9625 -1.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at -14.9625 -0.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -14.9625 -0.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -14.9625 0.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -14.9625 0.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -14.9625 1.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -14.9625 1.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -14.9625 2.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -14.9625 2.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at -14.9625 3.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at -14.9625 3.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at -14.9625 4.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -14.9625 4.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at -14.9625 5.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at -14.9625 5.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at -14.9625 6.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at -14.9625 6.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at -14.9625 7.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at -14.9625 7.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at -14.9625 8.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at -14.9625 8.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at -14.9625 9.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at -14.9625 9.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at -14.9625 10.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at -14.9625 10.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at -14.9625 11.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at -14.9625 11.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at -14.9625 12.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at -14.9625 12.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at -12.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at -12.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at -11.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at -11.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd roundrect
		(at -10.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "58" smd roundrect
		(at -10.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "59" smd roundrect
		(at -9.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "60" smd roundrect
		(at -9.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "61" smd roundrect
		(at -8.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "62" smd roundrect
		(at -8.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "63" smd roundrect
		(at -7.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "64" smd roundrect
		(at -7.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "65" smd roundrect
		(at -6.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "66" smd roundrect
		(at -6.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "67" smd roundrect
		(at -5.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "68" smd roundrect
		(at -5.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "69" smd roundrect
		(at -4.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "70" smd roundrect
		(at -4.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "71" smd roundrect
		(at -3.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "72" smd roundrect
		(at -3.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "73" smd roundrect
		(at -2.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "74" smd roundrect
		(at -2.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "75" smd roundrect
		(at -1.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "76" smd roundrect
		(at -1.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "77" smd roundrect
		(at -0.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "78" smd roundrect
		(at -0.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "79" smd roundrect
		(at 0.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "80" smd roundrect
		(at 0.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "81" smd roundrect
		(at 1.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "82" smd roundrect
		(at 1.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "83" smd roundrect
		(at 2.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "84" smd roundrect
		(at 2.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "85" smd roundrect
		(at 3.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "86" smd roundrect
		(at 3.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "87" smd roundrect
		(at 4.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "88" smd roundrect
		(at 4.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "89" smd roundrect
		(at 5.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "90" smd roundrect
		(at 5.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "91" smd roundrect
		(at 6.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "92" smd roundrect
		(at 6.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "93" smd roundrect
		(at 7.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "94" smd roundrect
		(at 7.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "95" smd roundrect
		(at 8.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "96" smd roundrect
		(at 8.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "97" smd roundrect
		(at 9.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "98" smd roundrect
		(at 9.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "99" smd roundrect
		(at 10.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "100" smd roundrect
		(at 10.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "101" smd roundrect
		(at 11.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "102" smd roundrect
		(at 11.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 12.25 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "104" smd roundrect
		(at 12.75 14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "105" smd roundrect
		(at 14.9625 12.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "106" smd roundrect
		(at 14.9625 12.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "107" smd roundrect
		(at 14.9625 11.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "108" smd roundrect
		(at 14.9625 11.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "109" smd roundrect
		(at 14.9625 10.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "110" smd roundrect
		(at 14.9625 10.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "111" smd roundrect
		(at 14.9625 9.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "112" smd roundrect
		(at 14.9625 9.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "113" smd roundrect
		(at 14.9625 8.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "114" smd roundrect
		(at 14.9625 8.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "115" smd roundrect
		(at 14.9625 7.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "116" smd roundrect
		(at 14.9625 7.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "117" smd roundrect
		(at 14.9625 6.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "118" smd roundrect
		(at 14.9625 6.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "119" smd roundrect
		(at 14.9625 5.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "120" smd roundrect
		(at 14.9625 5.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "121" smd roundrect
		(at 14.9625 4.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "122" smd roundrect
		(at 14.9625 4.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "123" smd roundrect
		(at 14.9625 3.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "124" smd roundrect
		(at 14.9625 3.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "125" smd roundrect
		(at 14.9625 2.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "126" smd roundrect
		(at 14.9625 2.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "127" smd roundrect
		(at 14.9625 1.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "128" smd roundrect
		(at 14.9625 1.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "129" smd roundrect
		(at 14.9625 0.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "130" smd roundrect
		(at 14.9625 0.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "131" smd roundrect
		(at 14.9625 -0.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "132" smd roundrect
		(at 14.9625 -0.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "133" smd roundrect
		(at 14.9625 -1.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "134" smd roundrect
		(at 14.9625 -1.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "135" smd roundrect
		(at 14.9625 -2.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "136" smd roundrect
		(at 14.9625 -2.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "137" smd roundrect
		(at 14.9625 -3.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "138" smd roundrect
		(at 14.9625 -3.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "139" smd roundrect
		(at 14.9625 -4.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "140" smd roundrect
		(at 14.9625 -4.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "141" smd roundrect
		(at 14.9625 -5.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "142" smd roundrect
		(at 14.9625 -5.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "143" smd roundrect
		(at 14.9625 -6.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "144" smd roundrect
		(at 14.9625 -6.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "145" smd roundrect
		(at 14.9625 -7.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "146" smd roundrect
		(at 14.9625 -7.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "147" smd roundrect
		(at 14.9625 -8.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "148" smd roundrect
		(at 14.9625 -8.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "149" smd roundrect
		(at 14.9625 -9.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "150" smd roundrect
		(at 14.9625 -9.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "151" smd roundrect
		(at 14.9625 -10.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "152" smd roundrect
		(at 14.9625 -10.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "153" smd roundrect
		(at 14.9625 -11.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "154" smd roundrect
		(at 14.9625 -11.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "155" smd roundrect
		(at 14.9625 -12.25)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "156" smd roundrect
		(at 14.9625 -12.75)
		(size 1.475 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "157" smd roundrect
		(at 12.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "158" smd roundrect
		(at 12.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "159" smd roundrect
		(at 11.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "160" smd roundrect
		(at 11.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "161" smd roundrect
		(at 10.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "162" smd roundrect
		(at 10.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "163" smd roundrect
		(at 9.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "164" smd roundrect
		(at 9.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "165" smd roundrect
		(at 8.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "166" smd roundrect
		(at 8.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "167" smd roundrect
		(at 7.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "168" smd roundrect
		(at 7.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "169" smd roundrect
		(at 6.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "170" smd roundrect
		(at 6.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "171" smd roundrect
		(at 5.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "172" smd roundrect
		(at 5.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "173" smd roundrect
		(at 4.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "174" smd roundrect
		(at 4.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "175" smd roundrect
		(at 3.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "176" smd roundrect
		(at 3.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "177" smd roundrect
		(at 2.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "178" smd roundrect
		(at 2.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "179" smd roundrect
		(at 1.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "180" smd roundrect
		(at 1.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "181" smd roundrect
		(at 0.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "182" smd roundrect
		(at 0.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "183" smd roundrect
		(at -0.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "184" smd roundrect
		(at -0.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "185" smd roundrect
		(at -1.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "186" smd roundrect
		(at -1.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "187" smd roundrect
		(at -2.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "188" smd roundrect
		(at -2.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "189" smd roundrect
		(at -3.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "190" smd roundrect
		(at -3.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "191" smd roundrect
		(at -4.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "192" smd roundrect
		(at -4.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "193" smd roundrect
		(at -5.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "194" smd roundrect
		(at -5.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "195" smd roundrect
		(at -6.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "196" smd roundrect
		(at -6.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "197" smd roundrect
		(at -7.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "198" smd roundrect
		(at -7.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "199" smd roundrect
		(at -8.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "200" smd roundrect
		(at -8.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "201" smd roundrect
		(at -9.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "202" smd roundrect
		(at -9.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "203" smd roundrect
		(at -10.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "204" smd roundrect
		(at -10.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "205" smd roundrect
		(at -11.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "206" smd roundrect
		(at -11.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "207" smd roundrect
		(at -12.25 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "208" smd roundrect
		(at -12.75 -14.9625)
		(size 0.3 1.475)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-208_28x28mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
