(footprint "PQFP-256_28x28mm_P0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PQFP256 28x28 / QFP256J CASE 122BX (see ON Semiconductor 122BX.PDF)")
	(tags "QFP 0.4")
	(property "Reference" "REF**"
		(at 0 -16.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "PQFP-256_28x28mm_P0.4mm"
		(at 0 16.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -15 -12.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -15 -12.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -15 -11.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -15 -11.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -15 -11)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -15 -10.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -15 -10.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -15 -9.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -15 -9.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -15 -9)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -15 -8.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -15 -8.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -15 -7.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -15 -7.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -15 -7)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -15 -6.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -15 -6.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -15 -5.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -15 -5.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -15 -5)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -15 -4.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -15 -4.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -15 -3.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -15 -3.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -15 -3)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -15 -2.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -15 -2.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -15 -1.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -15 -1.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -15 -1)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -15 -0.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -15 -0.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -15 0.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -15 0.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -15 1)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -15 1.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -15 1.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at -15 2.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -15 2.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -15 3)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -15 3.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at -15 3.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -15 4.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -15 4.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -15 5)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -15 5.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -15 5.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -15 6.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at -15 6.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at -15 7)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at -15 7.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at -15 7.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at -15 8.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at -15 8.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -15 9)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -15 9.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -15 9.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -15 10.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -15 10.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at -15 11)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at -15 11.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at -15 11.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at -15 12.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at -15 12.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at -12.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at -12.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at -11.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at -11.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at -11 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at -10.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at -10.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at -9.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at -9.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at -9 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at -8.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at -8.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at -7.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at -7.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at -7 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at -6.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at -6.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at -5.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at -5.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at -5 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at -4.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at -4.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd rect
		(at -3.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd rect
		(at -3.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd rect
		(at -3 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd rect
		(at -2.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd rect
		(at -2.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd rect
		(at -1.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd rect
		(at -1.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd rect
		(at -1 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd rect
		(at -0.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd rect
		(at -0.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd rect
		(at 0.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd rect
		(at 0.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd rect
		(at 1 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd rect
		(at 1.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd rect
		(at 1.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd rect
		(at 2.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd rect
		(at 2.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd rect
		(at 3 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd rect
		(at 3.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd rect
		(at 3.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd rect
		(at 4.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd rect
		(at 4.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd rect
		(at 5 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd rect
		(at 5.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd rect
		(at 5.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd rect
		(at 6.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd rect
		(at 6.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd rect
		(at 7 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd rect
		(at 7.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd rect
		(at 7.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd rect
		(at 8.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd rect
		(at 8.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd rect
		(at 9 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd rect
		(at 9.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd rect
		(at 9.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd rect
		(at 10.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd rect
		(at 10.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd rect
		(at 11 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd rect
		(at 11.4 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "126" smd rect
		(at 11.8 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "127" smd rect
		(at 12.2 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "128" smd rect
		(at 12.6 15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "129" smd rect
		(at 15 12.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "130" smd rect
		(at 15 12.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "131" smd rect
		(at 15 11.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "132" smd rect
		(at 15 11.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "133" smd rect
		(at 15 11)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "134" smd rect
		(at 15 10.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "135" smd rect
		(at 15 10.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "136" smd rect
		(at 15 9.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "137" smd rect
		(at 15 9.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "138" smd rect
		(at 15 9)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "139" smd rect
		(at 15 8.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "140" smd rect
		(at 15 8.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "141" smd rect
		(at 15 7.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "142" smd rect
		(at 15 7.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "143" smd rect
		(at 15 7)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "144" smd rect
		(at 15 6.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "145" smd rect
		(at 15 6.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "146" smd rect
		(at 15 5.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "147" smd rect
		(at 15 5.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "148" smd rect
		(at 15 5)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "149" smd rect
		(at 15 4.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "150" smd rect
		(at 15 4.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "151" smd rect
		(at 15 3.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "152" smd rect
		(at 15 3.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "153" smd rect
		(at 15 3)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "154" smd rect
		(at 15 2.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "155" smd rect
		(at 15 2.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "156" smd rect
		(at 15 1.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "157" smd rect
		(at 15 1.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "158" smd rect
		(at 15 1)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "159" smd rect
		(at 15 0.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "160" smd rect
		(at 15 0.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "161" smd rect
		(at 15 -0.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "162" smd rect
		(at 15 -0.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "163" smd rect
		(at 15 -1)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "164" smd rect
		(at 15 -1.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "165" smd rect
		(at 15 -1.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "166" smd rect
		(at 15 -2.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "167" smd rect
		(at 15 -2.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "168" smd rect
		(at 15 -3)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "169" smd rect
		(at 15 -3.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "170" smd rect
		(at 15 -3.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "171" smd rect
		(at 15 -4.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "172" smd rect
		(at 15 -4.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "173" smd rect
		(at 15 -5)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "174" smd rect
		(at 15 -5.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "175" smd rect
		(at 15 -5.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "176" smd rect
		(at 15 -6.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "177" smd rect
		(at 15 -6.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "178" smd rect
		(at 15 -7)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "179" smd rect
		(at 15 -7.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "180" smd rect
		(at 15 -7.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "181" smd rect
		(at 15 -8.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "182" smd rect
		(at 15 -8.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "183" smd rect
		(at 15 -9)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "184" smd rect
		(at 15 -9.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "185" smd rect
		(at 15 -9.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "186" smd rect
		(at 15 -10.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "187" smd rect
		(at 15 -10.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "188" smd rect
		(at 15 -11)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "189" smd rect
		(at 15 -11.4)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "190" smd rect
		(at 15 -11.8)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "191" smd rect
		(at 15 -12.2)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "192" smd rect
		(at 15 -12.6)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "193" smd rect
		(at 12.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "194" smd rect
		(at 12.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "195" smd rect
		(at 11.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "196" smd rect
		(at 11.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "197" smd rect
		(at 11 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "198" smd rect
		(at 10.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "199" smd rect
		(at 10.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "200" smd rect
		(at 9.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "201" smd rect
		(at 9.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "202" smd rect
		(at 9 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "203" smd rect
		(at 8.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "204" smd rect
		(at 8.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "205" smd rect
		(at 7.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "206" smd rect
		(at 7.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "207" smd rect
		(at 7 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "208" smd rect
		(at 6.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "209" smd rect
		(at 6.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "210" smd rect
		(at 5.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "211" smd rect
		(at 5.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "212" smd rect
		(at 5 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "213" smd rect
		(at 4.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "214" smd rect
		(at 4.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "215" smd rect
		(at 3.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "216" smd rect
		(at 3.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "217" smd rect
		(at 3 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "218" smd rect
		(at 2.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "219" smd rect
		(at 2.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "220" smd rect
		(at 1.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "221" smd rect
		(at 1.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "222" smd rect
		(at 1 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "223" smd rect
		(at 0.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "224" smd rect
		(at 0.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "225" smd rect
		(at -0.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "226" smd rect
		(at -0.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "227" smd rect
		(at -1 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "228" smd rect
		(at -1.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "229" smd rect
		(at -1.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "230" smd rect
		(at -2.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "231" smd rect
		(at -2.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "232" smd rect
		(at -3 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "233" smd rect
		(at -3.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "234" smd rect
		(at -3.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "235" smd rect
		(at -4.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "236" smd rect
		(at -4.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "237" smd rect
		(at -5 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "238" smd rect
		(at -5.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "239" smd rect
		(at -5.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "240" smd rect
		(at -6.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "241" smd rect
		(at -6.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "242" smd rect
		(at -7 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "243" smd rect
		(at -7.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "244" smd rect
		(at -7.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "245" smd rect
		(at -8.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "246" smd rect
		(at -8.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "247" smd rect
		(at -9 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "248" smd rect
		(at -9.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "249" smd rect
		(at -9.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "250" smd rect
		(at -10.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "251" smd rect
		(at -10.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "252" smd rect
		(at -11 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "253" smd rect
		(at -11.4 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "254" smd rect
		(at -11.8 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "255" smd rect
		(at -12.2 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "256" smd rect
		(at -12.6 -15 90)
		(size 1 0.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-256_28x28mm_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
