(footprint "TQFP-80-1EP_14x14mm_P0.65mm_EP9.5x9.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "80-Lead Plastic Thin Quad Flatpack (PF) - 14x14mm body, 9.5mm sq thermal pad (http://www.analog.com/media/en/technical-documentation/data-sheets/AD9852.pdf)")
	(tags "QFP 0.65")
	(property "Reference" "REF**"
		(at 0 -9.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "TQFP-80-1EP_14x14mm_P0.65mm_EP9.5x9.5mm"
		(at 0 9.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -2.375 -2.375)
		(size 3.8 3.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.375 2.375)
		(size 3.8 3.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.375 -2.375)
		(size 3.8 3.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.375 2.375)
		(size 3.8 3.8)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -7.7 -6.175)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -7.7 -5.525)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -7.7 -4.875)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -7.7 -4.225)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -7.7 -3.575)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -7.7 -2.925)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -7.7 -2.275)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -7.7 -1.625)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -7.7 -0.975)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -7.7 -0.325)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -7.7 0.325)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -7.7 0.975)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -7.7 1.625)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -7.7 2.275)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -7.7 2.925)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -7.7 3.575)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -7.7 4.225)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -7.7 4.875)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -7.7 5.525)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -7.7 6.175)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -6.175 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -5.525 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -4.875 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -4.225 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -3.575 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -2.925 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -2.275 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -1.625 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -0.975 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -0.325 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 0.325 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 0.975 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 1.625 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 2.275 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 2.925 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.575 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 4.225 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 4.875 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 5.525 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 6.175 7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 7.7 6.175)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 7.7 5.525)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 7.7 4.875)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 7.7 4.225)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 7.7 3.575)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 7.7 2.925)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 7.7 2.275)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 7.7 1.625)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 7.7 0.975)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 7.7 0.325)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 7.7 -0.325)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 7.7 -0.975)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 7.7 -1.625)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 7.7 -2.275)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 7.7 -2.925)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 7.7 -3.575)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 7.7 -4.225)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at 7.7 -4.875)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at 7.7 -5.525)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at 7.7 -6.175)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at 6.175 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at 5.525 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at 4.875 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at 4.225 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at 3.575 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at 2.925 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at 2.275 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at 1.625 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at 0.975 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at 0.325 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at -0.325 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at -0.975 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at -1.625 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at -2.275 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at -2.925 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at -3.575 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at -4.225 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at -4.875 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at -5.525 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at -6.175 -7.7 90)
		(size 1.5 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at 0 0)
		(size 9.5 9.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-80-1EP_14x14mm_P0.65mm_EP9.5x9.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
