(footprint "PowerIntegrations_eSIP-7C"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "eSIP-7C Vertical Flat Package with Heatsink Tab, https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf")
	(tags "Power Integrations E Package")
	(property "Reference" "REF**"
		(at 3.81 -2.2014 0)
		(layer "F.SilkS")
	)
	(property "Value" "PowerIntegrations_eSIP-7C"
		(at 3.81 5.0986 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.81 -0.2014 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.778 2.159)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 1.27 2.9972)
		(size 1.778 2.159)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 2.54 0)
		(size 1.778 2.159)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 3.81 2.9972)
		(size 1.778 2.159)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 5.08 0)
		(size 1.778 2.159)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 7.62 2.9972)
		(size 1.778 2.159)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SIP.3dshapes/PowerIntegrations_eSIP-7C.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
