(footprint "SIP4_Sharp-SSR_P7.62mm_Angled"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SIP4 Footprint for SSR made by Sharp")
	(tags "Solid State relais SSR Sharp")
	(property "Reference" "REF**"
		(at 1.27 -30.48 0)
		(layer "F.SilkS")
	)
	(property "Value" "SIP4_Sharp-SSR_P7.62mm_Angled"
		(at 7.62 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.62 -13.2 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 7.62 -26.2)
		(size 3.4 3.4)
		(drill 3.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 5.08 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 12.7 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 15.24 0)
		(size 2 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SIP.3dshapes/SIP4_Sharp-SSR_P7.62mm_Angled.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
