(footprint "HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HSOP 11.0x15.9mm Pitch 1.27mm Slug Down Thermal Vias (PowerSO-20) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/tda7266d.pdf, www.st.com/resource/en/application_note/cd00003801.pdf)")
	(tags "HSOP 11.0 x 15.9mm Pitch 1.27mm")
	(property "Reference" "REF**"
		(at 0 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown_ThermalVias"
		(at 0 9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.85 -5.715)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.85 -4.445)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.85 -3.175)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -6.85 -1.905)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -6.85 -0.635)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -6.85 0.635)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -6.85 1.905)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -6.85 3.175)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.85 4.445)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -6.85 5.715)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.85 5.715)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 6.85 4.445)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 6.85 3.175)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 6.85 1.905)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 6.85 0.635)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 6.85 -0.635)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 6.85 -1.905)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 6.85 -3.175)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 6.85 -4.445)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 6.85 -5.715)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" thru_hole circle
		(at -2.54 -2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -2.54 0)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -2.54 2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1.27 -5.08)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1.27 -2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1.27 0)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1.27 2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -1.27 5.08)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" smd rect
		(at 0 -6.8425)
		(size 3.4 2.415)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" thru_hole circle
		(at 0 -5.08)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 -2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 0)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" smd rect
		(at 0 0)
		(size 6.4 11.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0 0)
		(size 6.78 11.86)
		(layers "B.Cu")
	)
	(pad "21" thru_hole circle
		(at 0 2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 5.08)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" smd rect
		(at 0 6.8425)
		(size 3.4 2.415)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" thru_hole circle
		(at 1.27 -5.08)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1.27 -2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1.27 0)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1.27 2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 1.27 5.08)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 2.54 -2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 2.54 0)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 2.54 2.54)
		(size 1 1)
		(drill 0.7)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
