(footprint "HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugDown"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HSOP 11.0x15.9mm Pitch 0.65mm Slug Down (PowerSO-36) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/vn808cm-32-e.pdf, http://www.st.com/resource/en/application_note/cd00003801.pdf)")
	(tags "HSOP 11.0 x 15.9mm Pitch 0.65mm")
	(property "Reference" "REF**"
		(at 0 -9.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugDown"
		(at 0 9.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.85 -5.525)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.85 -4.875)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.85 -4.225)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -6.85 -3.575)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -6.85 -2.925)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -6.85 -2.275)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -6.85 -1.625)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -6.85 -0.975)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.85 -0.325)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -6.85 0.325)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -6.85 0.975)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -6.85 1.625)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -6.85 2.275)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -6.85 2.925)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -6.85 3.575)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -6.85 4.225)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -6.85 4.875)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -6.85 5.525)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 6.85 5.525)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 6.85 4.875)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 6.85 4.225)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 6.85 3.575)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 6.85 2.925)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 6.85 2.275)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 6.85 1.625)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 6.85 0.975)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 6.85 0.325)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 6.85 -0.325)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 6.85 -0.975)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 6.85 -1.625)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 6.85 -2.275)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 6.85 -2.925)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 6.85 -3.575)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 6.85 -4.225)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 6.85 -4.875)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 6.85 -5.525)
		(size 1.7 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 0 -8.125)
		(size 5 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 0 0)
		(size 9.4 14.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 0 8.125)
		(size 5 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugDown.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
