(footprint "HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16-Lead Plastic HTSSOP (4.4x5x1.2mm); Thermal pad with vias; (http://www.ti.com/lit/ds/symlink/drv8800.pdf)")
	(tags "SSOP 0.65")
	(property "Reference" "REF**"
		(at 0 -3.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias"
		(at 0 3.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.325 -0.55 90)
		(size 0.8 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.325 0.55 90)
		(size 0.8 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.55 -1.325)
		(size 0.8 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.55 -0.55)
		(size 0.85 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.55 0.55)
		(size 0.85 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.55 1.325)
		(size 0.8 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 3 3)
		(layers "F.Mask")
	)
	(pad "" smd rect
		(at 0.55 -1.325)
		(size 0.8 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.55 -0.55)
		(size 0.85 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.55 0.55)
		(size 0.85 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.55 1.325)
		(size 0.8 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.325 -0.55 90)
		(size 0.8 0.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.325 0.55 90)
		(size 0.8 0.25)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.775 -2.275)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.775 -1.625)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.775 -0.975)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.775 -0.325)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.775 0.325)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.775 0.975)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.775 1.625)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.775 2.275)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.775 2.275)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.775 1.625)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.775 0.975)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.775 0.325)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.775 -0.325)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.775 -0.975)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.775 -1.625)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.775 -2.275)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" thru_hole circle
		(at -1.1 -2.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at -1.1 -1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at -1.1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at -1.1 1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at -1.1 2.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 0 -2.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 0 -1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" smd rect
		(at 0 0)
		(size 3.4 5)
		(layers "F.Cu")
	)
	(pad "17" smd rect
		(at 0 0)
		(size 3.4 5)
		(layers "B.Cu")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" thru_hole circle
		(at 0 1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 0 2.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 1.1 -2.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 1.1 -1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 1.1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 1.1 1.1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 1.1 2.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16-1EP_4.4x5mm_Pitch0.65mm_EP3.4x5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
