(footprint "HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [HTSSOP], with thermal pad with vias")
	(tags "HTSSOP 0.65")
	(property "Reference" "REF**"
		(at 0 -4.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm"
		(at 0 4.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.85 -2.4375)
		(size 1.4 1.325)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.85 -0.8125)
		(size 1.4 1.325)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.85 0.8125)
		(size 1.4 1.325)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.85 2.4375)
		(size 1.4 1.325)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.85 -2.4375)
		(size 1.4 1.325)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.85 -0.8125)
		(size 1.4 1.325)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.85 0.8125)
		(size 1.4 1.325)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.85 2.4375)
		(size 1.4 1.325)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.95 -2.92)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.95 -2.27)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.95 -1.62)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.95 -0.97)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.95 -0.33)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.95 0.33)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.95 0.97)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.95 1.62)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -2.95 2.27)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.95 2.92)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.95 2.92)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.95 2.27)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.95 1.62)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.95 0.97)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.95 0.33)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.95 -0.33)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 2.95 -0.97)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 2.95 -1.62)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 2.95 -2.27)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.95 -2.92)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0 0)
		(size 3.4 6.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
