(footprint "HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm_Mask4.11x4.36mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HTSSOP32: plastic thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot487-1_po.pdf)")
	(tags "SSOP 0.65 PowerPAD")
	(property "Reference" "REF**"
		(at 0 -6.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm_Mask4.11x4.36mm"
		(at 0 6.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.37 -1.46)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.37 0)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.37 1.46)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -1.46)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 4.11 4.36)
		(layers "F.Mask")
	)
	(pad "" smd rect
		(at 0 1.46)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.37 -1.46)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.37 0)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.37 1.46)
		(size 1.07 1.16)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -3.65 -4.875)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.65 -4.225)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.65 -3.575)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.65 -2.925)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.65 -2.275)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.65 -1.625)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.65 -0.975)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.65 -0.325)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.65 0.325)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -3.65 0.975)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.65 1.625)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.65 2.275)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.65 2.925)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -3.65 3.575)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -3.65 4.225)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3.65 4.875)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 3.65 4.875)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 3.65 4.225)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 3.65 3.575)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 3.65 2.925)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 3.65 2.275)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 3.65 1.625)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 3.65 0.975)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 3.65 0.325)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 3.65 -0.325)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 3.65 -0.975)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 3.65 -1.625)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 3.65 -2.275)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 3.65 -2.925)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 3.65 -3.575)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 3.65 -4.225)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 3.65 -4.875)
		(size 1.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 0 0)
		(size 5.2 11)
		(layers "F.Cu")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
