(footprint "HTSSOP-38-1EP_6.1x12.5mm_P0.65mm_EP5.2x12.5mm_Mask3.39x6.35mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "HTSSOP, 38 Pin (http://www.ti.com/lit/ds/symlink/tlc5951.pdf#page=46), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "HTSSOP SO TI-DAP/R-PDSO-G38")
	(property "Reference" "REF**"
		(at 0 -7.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "HTSSOP-38-1EP_6.1x12.5mm_P0.65mm_EP5.2x12.5mm_Mask3.39x6.35mm"
		(at 0 7.2 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.85 -2.12)
		(size 1.37 1.71)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "" smd roundrect
		(at -0.85 0)
		(size 1.37 1.71)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "" smd roundrect
		(at -0.85 2.12)
		(size 1.37 1.71)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "" smd rect
		(at 0 0)
		(size 3.39 6.35)
		(layers "F.Mask")
	)
	(pad "" smd roundrect
		(at 0.85 -2.12)
		(size 1.37 1.71)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "" smd roundrect
		(at 0.85 0)
		(size 1.37 1.71)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "" smd roundrect
		(at 0.85 2.12)
		(size 1.37 1.71)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "1" smd roundrect
		(at -3.7125 -5.85)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.7125 -5.2)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.7125 -4.55)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.7125 -3.9)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.7125 -3.25)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.7125 -2.6)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.7125 -1.95)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.7125 -1.3)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -3.7125 -0.65)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -3.7125 0)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -3.7125 0.65)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -3.7125 1.3)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -3.7125 1.95)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -3.7125 2.6)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -3.7125 3.25)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -3.7125 3.9)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -3.7125 4.55)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -3.7125 5.2)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -3.7125 5.85)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 3.7125 5.85)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 3.7125 5.2)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 3.7125 4.55)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 3.7125 3.9)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 3.7125 3.25)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 3.7125 2.6)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 3.7125 1.95)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 3.7125 1.3)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 3.7125 0.65)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 3.7125 0)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 3.7125 -0.65)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 3.7125 -1.3)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 3.7125 -1.95)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 3.7125 -2.6)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 3.7125 -3.25)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 3.7125 -3.9)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 3.7125 -4.55)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 3.7125 -5.2)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 3.7125 -5.85)
		(size 1.575 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd rect
		(at 0 0)
		(size 5.2 12.5)
		(property pad_prop_heatsink)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-38-1EP_6.1x12.5mm_P0.65mm_EP5.2x12.5mm_Mask3.39x6.35mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
