(footprint "HTSSOP-56-1EP_6.1x14mm_P0.5mm_EP3.61x6.35mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HTSSOP56: plastic thin shrink small outline package http://www.ti.com/lit/ds/symlink/drv8301.pdf")
	(tags "HTSSOP 0.5")
	(property "Reference" "REF**"
		(at 0 -8.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "HTSSOP-56-1EP_6.1x14mm_P0.5mm_EP3.61x6.35mm"
		(at 0 8.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.2034 -2.54)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2034 -1.27)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2034 0)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2034 1.27)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.2034 2.54)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -2.54)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -1.27)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 1.27)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 2.54)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2034 -2.54)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2034 -1.27)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2034 0)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2034 1.27)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.2034 2.54)
		(size 0.96 1.03)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -3.75 -6.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.75 -6.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.75 -5.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.75 -5.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.75 -4.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.75 -4.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.75 -3.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.75 -3.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.75 -2.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -3.75 -2.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.75 -1.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.75 -1.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.75 -0.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -3.75 -0.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -3.75 0.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3.75 0.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -3.75 1.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -3.75 1.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -3.75 2.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -3.75 2.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -3.75 3.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -3.75 3.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -3.75 4.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -3.75 4.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -3.75 5.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -3.75 5.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -3.75 6.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -3.75 6.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 3.75 6.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 3.75 6.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 3.75 5.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 3.75 5.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 3.75 4.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.75 4.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 3.75 3.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.75 3.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 3.75 2.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 3.75 2.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 3.75 1.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 3.75 1.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 3.75 0.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 3.75 0.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 3.75 -0.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 3.75 -0.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 3.75 -1.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 3.75 -1.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 3.75 -2.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 3.75 -2.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 3.75 -3.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 3.75 -3.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 3.75 -4.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 3.75 -4.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 3.75 -5.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 3.75 -5.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 3.75 -6.25)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 3.75 -6.75)
		(size 1.55 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 0 0)
		(size 3.61 6.35)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-56-1EP_6.1x14mm_P0.5mm_EP3.61x6.35mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
