(footprint "Infineon_PG-DSO-12-9_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-9/)")
	(tags "PG-DSO")
	(property "Reference" "REF**"
		(at -3 -5.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-DSO-12-9_ThermalVias"
		(at 0 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.925 -2.92)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.925 -1.46)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.925 0)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.925 1.46)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.925 2.92)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.925 -2.92)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.925 -1.46)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.925 0)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.925 1.46)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.925 2.92)
		(size 1.55 1.16)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -4.8 -2.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.8 -1.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.8 -0.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.8 0.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.8 1.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.8 2.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 4.8 2.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.8 1.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 4.8 0.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.8 -0.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.8 -1.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 4.8 -2.5)
		(size 2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" thru_hole circle
		(at -1.85 -3.65)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -1.85 -2.19)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -1.85 -0.73)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -1.85 0.73)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -1.85 2.19)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at -1.85 3.65)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 -3.65)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 -2.19)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 -0.73)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" smd rect
		(at 0 0)
		(size 4.5 8.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd rect
		(at 0 0)
		(size 4.5 8.1)
		(layers "B.Cu")
	)
	(pad "13" thru_hole circle
		(at 0 0.73)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 2.19)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 3.65)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 1.85 -3.65)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 1.85 -2.19)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 1.85 -0.73)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 1.85 0.73)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 1.85 2.19)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 1.85 3.65)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Infineon_PG-DSO-12-9.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
