(footprint "Infineon_PG-DSO-20-30_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon SO package 20pin, exposed pad 4.5x7mm (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-71/)")
	(tags "DSO-20")
	(property "Reference" "REF**"
		(at 0 -7.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-DSO-20-30_ThermalVias"
		(at 0 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1 -2.325)
		(size 1.7 1.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1 -0.775)
		(size 1.7 1.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1 0.775)
		(size 1.7 1.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1 2.325)
		(size 1.7 1.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1 -2.325)
		(size 1.7 1.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1 -0.775)
		(size 1.7 1.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1 0.775)
		(size 1.7 1.25)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1 2.325)
		(size 1.7 1.25)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -4.75 -5.715 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.75 -4.445 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.75 -3.175 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.75 -1.905 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.75 -0.635 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.75 0.635 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.75 1.905 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.75 3.175 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -4.75 4.445 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -4.75 5.715 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.75 5.715 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 4.75 4.445 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 4.75 3.175 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 4.75 1.905 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 4.75 0.635 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 4.75 -0.635 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 4.75 -1.905 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 4.75 -3.175 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 4.75 -4.445 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 4.75 -5.715 90)
		(size 0.55 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" thru_hole circle
		(at -2 -3.1)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -2 -1.55)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -2 0)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -2 1.55)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at -2 3.1)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 -3.1)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 -1.55)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 0)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" smd rect
		(at 0 0)
		(size 4.8 7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd rect
		(at 0 0)
		(size 4.8 7)
		(layers "B.Cu")
	)
	(pad "21" thru_hole circle
		(at 0 1.55)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 0 3.1)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 2 -3.1)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 2 -1.55)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 2 0)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 2 1.55)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 2 3.1)
		(size 0.8 0.8)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Infineon_PG-DSO-20-30.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
