(footprint "Infineon_PG-DSO-20-85_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon SO package 20pin with exposed pad (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-85/)")
	(tags "DSO-20")
	(property "Reference" "REF**"
		(at 0 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-DSO-20-85_ThermalVias"
		(at 0 9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.4 -4.95)
		(size 2.4 2.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 -1.65)
		(size 2.4 2.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 1.65)
		(size 2.4 2.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.4 4.95)
		(size 2.4 2.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -7.36)
		(size 3.2 1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 7.36)
		(size 3.2 1)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 -4.95)
		(size 2.4 2.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 -1.65)
		(size 2.4 2.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 1.65)
		(size 2.4 2.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 4.95)
		(size 2.4 2.8)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -6.865 -5.715)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" thru_hole circle
		(at -2 -6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 -5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 -4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 -2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -2 6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 -7)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 -6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 -5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 -4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 -2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -1 7)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -7)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 7)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 7)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 -7)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 -6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 -5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 -4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 -2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 1 7)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 -6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 -5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 -4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 -2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 -1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 1)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2 6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" smd rect
		(at -6.865 -4.445)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.865 -3.175)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -6.865 -1.905)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -6.865 -0.635)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -6.865 0.635)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -6.865 1.905)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -6.865 3.175)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.865 4.445)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -6.865 5.715)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.865 5.715)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 6.865 4.445)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 6.865 3.175)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 6.865 1.905)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 6.865 0.635)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 6.865 -0.635)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 6.865 -1.905)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 6.865 -3.175)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 6.865 -4.445)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 6.865 -5.715)
		(size 1.83 0.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd custom
		(at 0 0)
		(size 5.9 13.7)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.6 7.87) (xy -1.6 7.87) (xy -1.6 -7.87) (xy 1.6 -7.87)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Infineon_PG-DSO-20-85.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
