(footprint "Infineon_PG-DSO-8-27_3.9x4.9mm_EP2.65x3mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Infineon  PG-DSO, 8 Pin (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-8-27), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "Infineon PG-DSO SO")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-DSO-8-27_3.9x4.9mm_EP2.65x3mm_ThermalVias"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.66 -0.75)
		(size 1.11 1.25)
		(layers "F.Paste")
		(roundrect_rratio 0.225225)
	)
	(pad "" smd roundrect
		(at -0.66 0.75)
		(size 1.11 1.25)
		(layers "F.Paste")
		(roundrect_rratio 0.225225)
	)
	(pad "" smd roundrect
		(at 0.66 -0.75)
		(size 1.11 1.25)
		(layers "F.Paste")
		(roundrect_rratio 0.225225)
	)
	(pad "" smd roundrect
		(at 0.66 0.75)
		(size 1.11 1.25)
		(layers "F.Paste")
		(roundrect_rratio 0.225225)
	)
	(pad "1" smd roundrect
		(at -2.625 -1.905)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.625 -0.635)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.625 0.635)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.625 1.905)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.625 1.905)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.625 0.635)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.625 -0.635)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.625 -1.905)
		(size 1.65 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" thru_hole circle
		(at -1.075 -1.25)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -1.075 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -1.075 1.25)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 -1.25)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 2.65 3)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 2.65 3)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "9" thru_hole circle
		(at 0 1.25)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 1.075 -1.25)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 1.075 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 1.075 1.25)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Infineon_PG-DSO-8-27_3.9x4.9mm_EP2.65x3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
