(footprint "Infineon_PG-DSO-8-43"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon_PG-DSO-8-43")
	(tags "DSO DSO-8 SOIC SOIC-8")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-DSO-8-43"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.845 -1.905)
		(size 1.31 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.845 -0.635)
		(size 1.31 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.845 0.635)
		(size 1.31 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.845 1.905)
		(size 1.31 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.845 1.905)
		(size 1.31 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.845 0.635)
		(size 1.31 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.845 -0.635)
		(size 1.31 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.845 -1.905)
		(size 1.31 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -0.6625 -0.75)
		(size 1.325 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at -0.6625 0.75)
		(size 1.325 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at 0.6625 -0.75)
		(size 1.325 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at 0.6625 0.75)
		(size 1.325 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Infineon_PG-DSO-8-43.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
