(footprint "Infineon_PG-TSDSO-14-22"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon_PG-TSDSO-14-22")
	(tags "Infineon TSDSO 14-22 ")
	(property "Reference" "REF**"
		(at 0 -3.556 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-TSDSO-14-22"
		(at 0 3.556 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at 0 -1.075)
		(size 2.65 1.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 1.075)
		(size 2.65 1.85)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.85 -1.95)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.85 -1.3)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.85 -0.65)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.845 0)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.85 0.65)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.85 1.3)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.85 1.95)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.85 1.95)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.85 1.3)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.85 0.65)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.85 0)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.85 -0.65)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.85 -1.3)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.85 -1.95)
		(size 1.31 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0 0)
		(size 2.65 4)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Infineon_PG-TSDSO-14-22.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
