(footprint "Linear_HTSSOP-31-38-1EP_4.4x9.7mm_P0.5mm_EP2.74x4.75mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Linear  HTSSOP, 31 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-tssop/tssop_38_05-08-1865.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "Linear HTSSOP SO FE38-(31)")
	(property "Reference" "REF**"
		(at 0 -5.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Linear_HTSSOP-31-38-1EP_4.4x9.7mm_P0.5mm_EP2.74x4.75mm"
		(at 0 5.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.685 -1.58)
		(size 1.1 1.28)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -0.685 0)
		(size 1.1 1.28)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at -0.685 1.58)
		(size 1.1 1.28)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 0.685 -1.58)
		(size 1.1 1.28)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 0.685 0)
		(size 1.1 1.28)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "" smd roundrect
		(at 0.685 1.58)
		(size 1.1 1.28)
		(layers "F.Paste")
		(roundrect_rratio 0.227273)
	)
	(pad "1" smd roundrect
		(at -2.775 -4.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.775 -4)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.775 -3.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.775 -3)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.775 -2.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.775 -2)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.775 -1.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -2.775 -1)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -2.775 -0.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -2.775 0)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -2.775 0.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -2.775 1)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -2.775 1.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -2.775 2)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -2.775 2.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -2.775 3)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -2.775 3.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -2.775 4)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -2.775 4.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.775 4.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.775 4)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 2.775 3.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.775 2.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 2.775 1.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 2.775 0.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 2.775 -0.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 2.775 -1.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 2.775 -2.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 2.775 -3.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 2.775 -4)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 2.775 -4.5)
		(size 1.05 0.315)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd rect
		(at 0 0)
		(size 2.74 4.75)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Linear_HTSSOP-31-38-1EP_4.4x9.7mm_P0.5mm_EP2.74x4.75mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
