(footprint "MFSOP6-4_4.4x3.6mm_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
	(tags "MFSOP 4 pin SMD")
	(property "Reference" "REF**"
		(at 0 -2.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "MFSOP6-4_4.4x3.6mm_P1.27mm"
		(at 0 2.921 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.15 -1.27)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.15 1.27)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.15 1.27)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3.15 -1.27)
		(size 1.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
