(footprint "NXP_HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.2x3.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HTSSOP, 28 Pin (https://www.nxp.com/docs/en/package-information/SOT1172-3.pdf)")
	(tags "HTSSOP SO")
	(property "Reference" "REF**"
		(at 0 -5.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "NXP_HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.2x3.4mm"
		(at 0 5.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.7 -1.23)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.7 -0.41)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.7 0.41)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.7 1.23)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 -1.23)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 -0.41)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 0.41)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 1.23)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.7 -1.23)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.7 -0.41)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.7 0.41)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.7 1.23)
		(size 0.6 0.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -3.05 -4.325)
		(size 1.35 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "2" smd roundrect
		(at -3.05 -3.575)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.05 -2.925)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.05 -2.275)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.05 -1.625)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.05 -0.975)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.05 -0.325)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.05 0.325)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -3.05 0.975)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -3.05 1.625)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -3.05 2.275)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -3.05 2.925)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -3.05 3.575)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -3.05 4.325)
		(size 1.35 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "15" smd roundrect
		(at 3.05 4.325)
		(size 1.35 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "16" smd roundrect
		(at 3.05 3.575)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 3.05 2.925)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 3.05 2.275)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 3.05 1.625)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 3.05 0.975)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 3.05 0.325)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 3.05 -0.325)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 3.05 -0.975)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 3.05 -1.625)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 3.05 -2.275)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 3.05 -2.925)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 3.05 -3.575)
		(size 1.35 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 3.05 -4.325)
		(size 1.35 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "29" smd rect
		(at 0 0)
		(size 2.2 3.4)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/NXP_HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.2x3.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
