(footprint "ONSemi_SO-8FL_488AA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ON Semi DFN5 5x6mm 1.27P SO-8FL CASE 488A https://www.onsemi.com/pub/Collateral/488AA.PDF")
	(tags "ON Semi DFN5 5x6mm 1.27P SO-8FL CASE 488A ")
	(property "Reference" "REF**"
		(at 0 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "ONSemi_SO-8FL_488AA"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.04775 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.74725 -1.905)
		(size 1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.74725 -0.635)
		(size 1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.74725 0.635)
		(size 1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.74725 1.905)
		(size 1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at 0.745 0)
		(size 4.055 4.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.6975 -2.28) (xy 2.5025 -2.28) (xy 2.5025 -1.53) (xy 1.905 -1.53) (xy 1.905 1.53) (xy 2.5025 1.53)
					(xy 2.5025 2.28) (xy -0.6975 2.28) (xy -0.6975 2.775) (xy -1.6025 2.775) (xy -1.6025 -2.775) (xy -0.6975 -2.775)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/ONSemi_SO-8FL_488AA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
