(footprint "PSOP-44_16.9x27.17mm_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PSOP44: plastic thin shrink small outline package; 44 leads; body width 16.90 mm")
	(tags "PSOP 1.27")
	(property "Reference" "REF**"
		(at 0 -15.285 0)
		(layer "F.SilkS")
	)
	(property "Value" "PSOP-44_16.9x27.17mm_P1.27mm"
		(at 0 15.24 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -8 -13.335 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8 -12.065 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -8 -10.795 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -8 -9.525 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -8 -8.255 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -8 -6.985 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8 -5.715 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8 -4.445 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -8 -3.175 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -8 -1.905 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -8 -0.635 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -8 0.635 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -8 1.905 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -8 3.175 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -8 4.445 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -8 5.715 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -8 6.985 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -8 8.255 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -8 9.525 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -8 10.795 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -8 12.065 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -8 13.335 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 8 13.335 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 8 12.065 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 8 10.795 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 8 9.525 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 8 8.255 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 8 6.985 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 8 5.715 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 8 4.445 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 8 3.175 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 8 1.905 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 8 0.635 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 8 -0.635 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 8 -1.905 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 8 -3.175 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 8 -4.445 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 8 -5.715 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 8 -6.985 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 8 -8.255 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 8 -9.525 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 8 -10.795 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 8 -12.065 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 8 -13.335 270)
		(size 0.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/PSOP-44_16.9x27.17mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
