(footprint "SOIC-16W-12_7.5x10.3mm_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOIC-16 With 12 Pin Placed - Wide, 7.50 mm Body [SOIC] (https://docs.broadcom.com/docs/AV02-0169EN)")
	(tags "SOIC 1.27 16 12 Wide")
	(property "Reference" "REF**"
		(at 0 -6.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOIC-16W-12_7.5x10.3mm_P1.27mm"
		(at 0 6.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.65 -4.445)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.65 -3.175)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.65 -1.905)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.65 1.905)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.65 3.175)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.65 4.445)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 4.65 4.445)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.65 3.175)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.65 1.905)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 4.65 -1.905)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 4.65 -3.175)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 4.65 -4.445)
		(size 1.5 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W-12_7.5x10.3mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
