(footprint "SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SOIC, 8 Pin (https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP2303A/document_id/494#page=14), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOIC SO")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.655 -0.875)
		(size 1.06 1.41)
		(layers "F.Paste")
		(roundrect_rratio 0.235849)
	)
	(pad "" smd roundrect
		(at -0.655 0.875)
		(size 1.06 1.41)
		(layers "F.Paste")
		(roundrect_rratio 0.235849)
	)
	(pad "" smd roundrect
		(at 0.655 -0.875)
		(size 1.06 1.41)
		(layers "F.Paste")
		(roundrect_rratio 0.235849)
	)
	(pad "" smd roundrect
		(at 0.655 0.875)
		(size 1.06 1.41)
		(layers "F.Paste")
		(roundrect_rratio 0.235849)
	)
	(pad "1" smd roundrect
		(at -2.48 -1.905)
		(size 1.94 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.48 -0.635)
		(size 1.94 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.48 0.635)
		(size 1.94 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.48 1.905)
		(size 1.94 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.48 1.905)
		(size 1.94 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.48 0.635)
		(size 1.94 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.48 -0.635)
		(size 1.94 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.48 -1.905)
		(size 1.94 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 2.62 3.51)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
