(footprint "SOIC-8_5.3x5.3mm_P1.27mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SOIC, 8 Pin (JEITA/EIAJ 08-001-BBA and Atmel/Microchip, 208 mils width, https://www.jeita.or.jp/japanese/standard/book/ED-7311-19/#target/page_no=21, https://ww1.microchip.com/downloads/en/DeviceDoc/20005045C.pdf#page=23, https://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=162), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOIC SO P-SOP SOP SOP-8 SO SO-8 8S2 S2AE/F K04-056 CASE-751BE SO8W 8-Pin-SOIC PSA W8-2 W8-4 W8MS-1")
	(property "Reference" "REF**"
		(at 0 -3.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOIC-8_5.3x5.3mm_P1.27mm"
		(at 0 3.6 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.5875 -1.905)
		(size 1.625 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.5875 -0.635)
		(size 1.625 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.5875 0.635)
		(size 1.625 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.5875 1.905)
		(size 1.625 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.5875 1.905)
		(size 1.625 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 3.5875 0.635)
		(size 1.625 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 3.5875 -0.635)
		(size 1.625 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 3.5875 -1.905)
		(size 1.625 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_5.3x5.3mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
