(footprint "SOP-8_3.76x4.96mm_P1.27mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SOP, 8 Pin (https://ww2.minicircuits.com/case_style/XX211.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOP SO")
	(property "Reference" "REF**"
		(at 0 -3.43 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOP-8_3.76x4.96mm_P1.27mm"
		(at 0 3.43 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.5375 -1.905)
		(size 1.975 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.5375 -0.635)
		(size 1.975 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.5375 0.635)
		(size 1.975 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.5375 1.905)
		(size 1.975 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.5375 1.905)
		(size 1.975 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.5375 0.635)
		(size 1.975 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.5375 -0.635)
		(size 1.975 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.5375 -1.905)
		(size 1.975 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.76x4.96mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
