(footprint "SSO-7-8_6.4x9.78mm_P2.54mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SSO, 7 Pin (https://b2b-api.panasonic.eu/file_stream/pids/fileversion/2787), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SSO SO")
	(property "Reference" "REF**"
		(at 0 -5.84 0)
		(layer "F.SilkS")
	)
	(property "Value" "SSO-7-8_6.4x9.78mm_P2.54mm"
		(at 0 5.84 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.3 -3.81)
		(size 1.85 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "2" smd roundrect
		(at -4.3 -1.27)
		(size 1.85 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "3" smd roundrect
		(at -4.3 1.27)
		(size 1.85 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "4" smd roundrect
		(at -4.3 3.81)
		(size 1.85 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "5" smd roundrect
		(at 4.3 3.81)
		(size 1.85 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "6" smd roundrect
		(at 4.3 1.27)
		(size 1.85 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(pad "8" smd roundrect
		(at 4.3 -3.81)
		(size 1.85 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.178571)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSO-7-8_6.4x9.78mm_P2.54mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
