(footprint "SSO-8_6.7x9.8mm_P2.54mm_Clearance8mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://www.vishay.com/docs/83831/lh1533ab.pdf")
	(tags "SSO Stretched SO SOIC Pitch 2.54")
	(property "Reference" "REF**"
		(at 0 -5.805 0)
		(layer "F.SilkS")
	)
	(property "Value" "SSO-8_6.7x9.8mm_P2.54mm_Clearance8mm"
		(at 0 6.005 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.76 -3.81)
		(size 1.52 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.76 -1.27)
		(size 1.52 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.76 1.27)
		(size 1.52 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.76 3.81)
		(size 1.52 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 4.76 3.81)
		(size 1.52 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 4.76 1.27)
		(size 1.52 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 4.76 -1.27)
		(size 1.52 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.76 -3.81)
		(size 1.52 1.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSO-8_6.7x9.8mm_P2.54mm_Clearance8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
