(footprint "SSOP-10-1EP_3.9x4.9mm_P1mm_EP2.1x3.3mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SSOP, 10 Pin (http://download.py32.org/%E6%95%B0%E6%8D%AE%E6%89%8B%E5%86%8C/zh-CN/PY32F002A%20%E7%B3%BB%E5%88%97%E6%95%B0%E6%8D%AE%E6%89%8B%E5%86%8C_Rev1.0.pdf#page=44), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SSOP SO ESSOP-10")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "SSOP-10-1EP_3.9x4.9mm_P1mm_EP2.1x3.3mm"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.69 2.66)
		(layers "F.Paste")
		(roundrect_rratio 0.147929)
	)
	(pad "1" smd roundrect
		(at -2.6375 -2)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.6375 -1)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.6375 0)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.6375 1)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.6375 2)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.6375 2)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.6375 1)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.6375 0)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 2.6375 -1)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 2.6375 -2)
		(size 1.675 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd rect
		(at 0 0)
		(size 2.1 3.3)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-10-1EP_3.9x4.9mm_P1mm_EP2.1x3.3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
